一、线缆类型：MIC1 to MIC8
所有线缆都需要进行样件认证，认证合格后再生产正式产品。
表1：线缆种类
	
	信号分类与电学特性
	MI线缆规格
	线缆耐压
测试

	用途
	额定电压(V)
	额定电流值(A)
	MIC#
	线缆外径（mm）
	端接头针芯数量
	端头数量
	测试电压(V)

	仪器（热电偶）
	50 
	0.5 
	MIC1
	1.5
	2
	2
	200

	仪器设备
	
	
	MIC1-hj
	1.5
	2
	1
	200

	仪器设备
	50
	0.5
	MIC2
	1.6
	2
	2
	200

	控制/电源线
	300 
	20 
	MIC3
	3
	1
	2
	1000

	
	
	
	MIC4
	6
	2
	2
	1000

	控制/电源线
	600 
	4
	MIC5
	3
	2
	2
	1200

	
	
	
	MIC6
	4
	4
	2
	1200

	控制/电源线
	1000 
	2
	MIC7
	3
	1
	2
	2000

	
	
	
	MIC8
	6.4
	4
	2
	2000



二、 ITER LEVI 矿物质绝缘（MI）线缆首批采购范围
表2：ITER LEVI 矿物质绝缘（MI）线缆首批采购范围
	序号
	产品描述
	产品型号
	线缆长度
	数量（根）
	线缆外径（mm）
	端接头针芯直径
(mm)
	端接头针芯数量
	端头数量

	1
	LEVI MI线缆
	MIC1
	015A
	2.710m±1cm
	10
	1.5
	　/
	2
	2

	2
	
	MIC1-hj
	015B
	2.735m ±1cm
	2
	1.5
	　/
	2
	1

	3
	
	MIC1-hj
	015B
	0.473m ±1cm
	4
	1.5
	　/
	2
	1

	4
	
	MIC1-hj
	015B
	0.261 ±1cm
	12
	1.5
	　/
	2
	1

	5
	
	MIC1-hj
	015B
	0.836 ±1cm
	21
	1.5
	　/
	2
	1

	6
	
	[bookmark: OLE_LINK17]MIC2
	016A
	0.6m ±1cm
	9
	1.6
	　/
	2
	2

	7
	
	MIC7
	030B
	0.434m ±1cm
	4
	3
	2.1
	1
	2

	8
	
	MIC5
	030C
	0.9m ±1cm
	4
	3
	1.2
	2
	2

	9
	
	MIC5
	030C
	1.915m ±1cm
	6
	3
	1.2
	2
	2

	10
	
	MIC6
	040A
	1.902m±1cm
	46
	4
	　/
	4
	2


备注：1.以上数量和尺寸是最终交付的做好接头之后的最终合格的交付数量和尺寸，总价包括生产过程中间的线缆和端头损耗。2.每种规格的线缆需额外生产1-2件用于测试的样件。3.每种规格的线缆最终交付长度可能与表2有所差异，以甲方最终需求为准。4.所有正式交付的线缆产品均以直线状态交付。

[bookmark: _GoBack]三、技术要求
3.1线缆总成要求
[RQ‑1] 线缆总成长度与标称长度公差：±10 mm。
[RQ‑2] 工厂验收试验 (FAT) 必须测量每根线缆总成长度，测量精度优于 ±2 mm。
[RQ‑3] 所有线缆总成的电气指标可参考表3，以甲方最终定稿版为准。



表3：线缆电气指标
	A
	B
	C
	D
	E
	F
	G
	H

	MIC#
	Rated Voltage
	Rated Current
	Withstand Voltage for Cables
(Dielectric strength)
	Insulation Resistance
(Room ambient
environmental conditions)
	Short-Circuit Current
value (A) – Values from
IEEE 317 Standard
	Short-Circuit Current
value(A) – if applicable
	Thermal Test (A2.t)

	MIC#1
	50 V
	0.5 A
	200V RMS test voltage @ 50Hz
	> 100 G Ω @ 300 VDC
	Not applicable
	Not applicable
	Not applicable

	MIC#1-hj
	50 V
	0.5 A
	200V RMS test voltage @ 50Hz
	> 100 G Ω @ 300 VDC
	Not applicable
	Not applicable
	Not applicable

	MIC#2
	50 V
	0.5 A
	200V RMS test voltage @ 50Hz
	> 100 G Ω @ 300 VDC
	Not applicable
	Not applicable
	Not applicable

	MIC#3
	300V
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	1000V RMS @ 50Hz
	> 100 G Ω @ 300 VDC
	858 A
	400 A
	11544 A2.t

	MIC#4
	300V
	20 A
	1000V RMS @ 50Hz
	> 100 G Ω @ 300 VDC
	945 A
	400 A
	14032 A2.t

	MIC#5
	600V
	4 A
	1200V RMS @ 50Hz
	> 100 G Ω @ 600 VDC
	111 A
	80 A
	190 A2.t

	MIC#6
	600V
	4 A
	1200V RMS @ 50Hz
	> 100 G Ω @ 600 VDC
	217 A
	80 A
	721 A2.t

	MIC#7
	1000V
	2 A
	2000V RMS @ 50Hz
	> 100 G Ω @ 1000 VDC
	485 A
	40 A
	3653 A2.t

	MIC#8
	1000V
	20A
	2000V RMS @ 50Hz
	> 100 G Ω @ 1000 VDC
	552 A
	40 A
	4728 A2.t







[RQ‑4] 线缆完成端接后应可直接进行弯曲作业。

