采购需求及技术规格要求
1、货物需求一览表
	序号
	货物名称
	数量
	型号规格
	图纸UID

	1
	[bookmark: OLE_LINK17]T型不锈钢锻件Semi-finished 316L(N)-IG forged T-shape bars
	123
	长度227mm
	FBMQ2B_v1

	2
	T型不锈钢锻件Semi-finished 316L(N)-IG forged T-shape bars 
	369
	长度275mm
	FBMQ2B_v1

	3
	T型不锈钢锻件Semi-finished 316L(N)-IG forged T-shape bars
	36
	长度347mm
	FBMQ2B_v1

	4
	铝青铜嵌件Inserts (CW307G bronze) M8X12_1.25_SPIRALOCK
	9
	见图纸
	AXB2GQ_v2

	5
	铝青铜嵌件Inserts (CW307G bronze) M8X12_1.25_SPIRALOCK customized for E2 QB
	24
	见图纸
	YQMKAP_v1

	6
	铝青铜嵌件Inserts (CW307G bronze) M10X15_12.75_SPIRALOCK
	56
	见图纸
	AXB2H8_v2

	7
	铝青铜夹紧销Clamping Pins (CW307G bronze) ISO 8752_6X14
	89
	ISO 8752_6*14
	/

	8
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø100X1000
	4
	Φ100*1000
	/

	9
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø60X1000
	10
	Φ60*1000
	/

	10
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø60X800
	1
	Φ60*800
	/

	11
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø40X1000
	3
	Φ40*1000
	/

	12
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø40X600
	1
	Φ40*600
	/

	13
	不锈钢棒材Semi-finished 316L(N)-IG stainless steel rods with circular cross-section Ø16X1000
	20
	Φ16*1000
	/
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